Minutes of RESULTS, PITZ Physics Seminar, 08.12.2011

Project: PITZ
Participants. Mikhail Krasilnikov, Georgios Kourkafas, Igor Isaev, Dmitriy Malyutin, Martin Khojoyan, Ji Li, Barbara Marchetti, Sakhorn Rimjaem, Marek Otevrel, Grigoriy Vashchenko, Davit Kalantaryan, Keerati Kusoljariyakul, Mahmoud Mahgoub, Mathias Gross, Frank Stephan, Anne Oppelt 

Agenda:
1)	Summary of HEDA2 and Preparation for Commissioning (S. Rimjaem)
2)	Acousto-optic Modulator (AOM) as Laser Pulse Picker (M. Gross)
3)	Summary of Proton-Driven PWA Meeting (M. Gross)

Results:
1)	
Next steps:
What is to be done?	By whom?	Until when?	Done on	
To set the current of dipole HEDA2.D2 and D3 to their calibration point if the calibration point of D1 is set in the control. And if the dipole D1 is set to zero (in degaussing) then D2 and D3 must be set to zero.	Control group, Keerati			
To check the effect of the fringe field on ICT and compare with the ICT at LEDA section.	Dieter Richter and Keerati	open		
To find how long the power supplies for HEDA2 magnets take to reach the set point.	Levon and Keerati			
The control should set the correct camera (OTR or YAG) for HEDA2.SCR1 automatically according to the screen in use.	D. Malyutin	?		
To find calibration data for ICT in HEDA1 and HEDA2.	Dieter Richter and Keerati	December 2011		
To test the stability of trigger box of AOM need long term test might need connection to master oscillator.	M. Gross			
To open BSA to see more of transverse profile.	M. Gross			
To do OSS measurement.	M. Gross	generally		

Protocol prepared by
Keerati Kusoljariyakul, 08.12.2011